24 KHz 25% duty Clock:

To implement the 25% duty cycle, we can leave LED on for 1 interrupt, off for 3 interrupts

24 KHz 50% duty Square Wave:

20 second 50% duty Square Wave:

By counting to 500 interrupts, we can implement a 20 second period without the counter rolling over.

2 Bit Timer: